Routing Protocol is "rip"
  Sending updates every 30 seconds with +/-50%, next due in XX seconds
  Timeout after 180 seconds, garbage collect after 120 seconds
  Outgoing update filter list for all interface is not set
  Incoming update filter list for all interface is not set
  Default redistribution metric is 1
  Redistributing:
  Default version control: send version 2, receive version 2 
    Interface        Send  Recv   Key-chain
    r1-eth1          2     2      
  Routing for Networks:
    192.168.1.0/26
  Routing Information Sources:
    Gateway          BadPackets BadRoutes  Distance Last Update
  Distance: (default is 120)
