Routing Protocol is "RIPng"
  Sending updates every 1 seconds with +/-50%, next due in XX seconds
  Timeout after 180 seconds, garbage collect after 5 seconds
  Outgoing update filter list for all interface is not set
  Incoming update filter list for all interface is not set
  Default redistribution metric is 1
  Redistributing:
  Default version control: send version 1, receive version 1 
    Interface        Send  Recv
    r2-eth0          1     1  
    r2-eth1          1     1  
  Routing for Networks:
    fc00:5::/64
    fc00:6::/62
  Routing Information Sources:
    Gateway          BadPackets BadRoutes  Distance Last Update
    fe80::XXXX:XXXX:XXXX:XXXX 
                        0          0        120      XX:XX:XX
    fe80::XXXX:XXXX:XXXX:XXXX 
                        0          0        120      XX:XX:XX
