## Color coding:
#########################
##  Main FRR: #f08080  red
##  Switches: #d0e0d0  gray
##  RIP:      #19e3d9  Cyan
##  RIPng:    #fcb314  dark yellow
##  OSPFv2:   #32b835  Green
##  OSPFv3:   #19e3d9  Cyan
##  ISIS IPv4 #fcb314  dark yellow
##  ISIS IPv6 #9a81ec  purple
##  BGP IPv4  #eee3d3  beige
##  BGP IPv6  #fdff00  yellow
##### Colors (see http://www.color-hex.com/)

graph bgp_vrf_netns_eBGP_topo1 {
	label="bgp vrf netns topo1 - eBGP with different AS numbers";
    labelloc="t";

	# Routers
	r1 [
		label="r1\nrtr-id 10.0.255.1/32",
		shape=doubleoctagon,
		fillcolor="#f08080",
		style=filled,
	];

	# 1 Switch for eBGP Peers
	s1 [
		label="s1\n10.0.1.0/24",
		shape=oval,
		fillcolor="#d0e0d0",
		style=filled,
	];

	# 1 ExaBGP Peers AS 101
	peer1 [
		label="eBGP peer1\nAS101\nrtr-id 10.0.1.101/32",
		shape=rectangle,
		fillcolor="#eee3d3",
		style=filled,
	];

	# Connections
	r1 -- s1 [label="eth0\n.1"];

	peer1 -- s1 [label="eth0\n.101"];

	# Arrange network to make cleaner diagram
	{ rank=same peer1 } -- s1 -- { rank=same r1 } [style=invis]
}
