## GraphViz file for test_rip_topo1
##
## Color coding:
#########################
##  Main FRR: #f08080  red
##  Switches: #d0e0d0  gray
##  RIP:      #19e3d9  Cyan
##  RIPng:    #fcb314  dark yellow
##  OSPFv2:   #32b835  Green
##  OSPFv3:   #19e3d9  Cyan
##  ISIS IPv4 #fcb314  dark yellow
##  ISIS IPv6 #9a81ec  purple
##  BGP IPv4  #eee3d3  beige
##  BGP IPv6  #fdff00  yellow
##### Colors (see http://www.color-hex.com/)

graph test_rip_topo1 {
	overlap=false;
	constraint=false;

    // title
    labelloc="t";
    label="Test Topologoy RIP Topo1";

	######################
	# Routers	
	######################

	# Main FRR Router with all protocols
	R1 [shape=doubleoctagon, label="R1 FRR\nMain Router", fillcolor="#f08080", style=filled];
	
	# RIP Routers
	R2 [shape=doubleoctagon, label="R2 FRR\nRIP Router", fillcolor="#19e3d9", style=filled];
	R3 [shape=doubleoctagon, label="R3 FRR\nRIP Router", fillcolor="#19e3d9", style=filled];

	######################
	# Network Lists
	######################

    SW1_R1_stub [label="SW1\n192.168.1.0/24", fillcolor="#d0e0d0", style=filled];

	# RIP Networks
    SW2_R1_R2 [label="SW2\nRIPv2\n193.1.1.0/26", fillcolor="#d0e0d0", style=filled];
    SW3_R2_R3 [label="SW3\nRIPv1\n193.1.2.0/24", fillcolor="#d0e0d0", style=filled];
    SW4_R3 [label="SW4\n192.168.3.0/24", fillcolor="#d0e0d0", style=filled];
    Net_R3_remote [label="Static Net\n192.168.2.0/24"];

	######################
	# Network Connections
	######################
    R1 -- SW1_R1_stub [label = "eth0\n.1\n::1"];

    # RIP Network
    R1 -- SW2_R1_R2 [label = "eth1\n.1"];
    SW2_R1_R2 -- R2 [label = "eth0\n.2"];
    R2 -- SW3_R2_R3 [label = "eth1\n.1"];
    SW3_R2_R3 -- R3 [label = "eth1\n.2"];
    R3 -- SW4_R3 [label = "eth0\n.1"];
    SW4_R3 -- Net_R3_remote [label = ".10"];
	
}
