// SPDX-License-Identifier: BSD-2-Clause
module frr-test-module {
  yang-version 1.1;
  namespace "urn:frr-test-module";
  prefix frr-test-module;

  import ietf-inet-types {
    prefix inet;
  }
  import frr-interface {
    prefix frr-interface;
  }

  organization "placeholder for lint";

  contact "placeholder for lint";

  description
    "FRRouting internal testing module.

     Copyright 2020 FRRouting

     Redistribution and use in source and binary forms, with or without
     modification, are permitted provided that the following conditions
     are met:

     1. Redistributions of source code must retain the above copyright notice,
     this list of conditions and the following disclaimer.

     2. Redistributions in binary form must reproduce the above copyright
     notice, this list of conditions and the following disclaimer in the
     documentation and/or other materials provided with the distribution.

     THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS
     \"AS IS\" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT
     LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR
     A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT
     HOLDER OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL,
     SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT
     LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE,
     DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY
     THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
     (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE
     OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.";

  revision 2018-11-26 {
    description
      "Initial revision.";
    reference "placeholder for lint";
  }

  container frr-test-module {
    config false;
    description "a container for test module data";
    container vrfs {
      description "a container of vrfs";
      list vrf {
        key "name";
        description "a keyed vrf list object";

        leaf name {
          type string;
          description "name of vrf";
        }
        container interfaces {
          description "container of leaf-list interfaces";
          leaf-list interface {
            type frr-interface:interface-ref;
            description "leaf list interface object";
          }
          leaf-list interface-new {
            type frr-interface:interface-ref;
            description "second leaf list interface object";
          }
        }
        container routes {
          description "container of key-less route objects";
          list route {
            description "a key-less route object";
            leaf prefix {
              type inet:ipv4-prefix;
              description "prefix of the route object";
            }
            leaf next-hop {
              type inet:ipv4-address;
              description "nexthop of the route object";
            }
            leaf interface {
              type frr-interface:interface-ref;
              description "interface of the route object";
            }
            leaf metric {
              type uint8;
              description "metric of the route object";
            }
            leaf active {
              type empty;
              description "active status of the route object";
            }
          }
        }
        action ping {
          input {
            leaf data {
              type string;
              description "data input to ping action.";
            }
          }
          output {
            leaf vrf {
              type string;
              description "vrf returned from ping action.";
            }
            // can't use the same name in input and output
            // because of a bug in libyang < 2.1.148
            leaf data-out {
              type string;
              description "data return from ping action.";
            }
          }
        }
      }
    }
    choice achoice {
      description "a choice statement";
      case case1 {
        leaf c1value {
          type uint8;
          description "A uint8 value for case 1";
        }
      }
      case case2 {
        container c2cont {
          description "case 2 container";
          leaf c2value {
            type uint32;
            description "A uint32 value for case 2";
          }
        }
      }
    }
  }
}
